BACKYARDS OF AMERICA

248 W 9240 S Sandy, UT 84070

Phone: 801-561-0679

Email: boa@backyardsofamerica.com

Website: [www.backyardsofamerica.com](http://www.backyardsofamerica.com)

**SPA CHEMISTRY FOR AN AQUA FINESSE SYSTEM**

\*Please turn on spa pumps when adding chemicals to your spa.

|  |
| --- |
| **Aqua Finesse Per Week** |
| **Gallons** | **Solution** |
| <250 | 6oz |
| 251-350 | 7oz |
| 351-450 | 10oz |
| 451-550 | 13oz |
| 551-650 | 14oz |

 **EVERY USE**

* **Add 1 scoop** of Granular Chlorine \****per person*** (Spa Boss or Spa 56)

**EVERY WEEK**

* **Test** **water** Chemistry (Alkalinity, pH, and Calcium Hardness)
* **Add** Spa Up *if pH is Low* (low pH is caustic and will attack materials in your spa)
* **Add** Spa Down *if pH is High* (high pH will cause calcium buildup on the heater and other parts)
* **Shake** Aqua Finesse Solution and **Add** according to chart above

\*Spray your filter with your hose every few weeks

 **EVERY DRAIN AND REFILL** \*(Recommended every 4-6 months)

* Use the Spa Clean (Puck) to purge water lines **BEFORE** draining old water
* **Deep clean** filter with filter cleaner tablets (2 per filter)

\*Continue with the EVERY WEEK checklist

* **Clean and treat** cover, pillows, and synthetic cabinet with 303

**OTHER**

* **Replace** main filter every 18-24 months
* **Replace** micro-clean filter every 4-6 months (on select models)
* **Replace** Clear Ray bulb every 12 months (on select models)

**-----------------------------------------------------------------------------------------------------------------------------------------**

We understand this may be a lot to remember. In order to better serve you, please check out our new IPhone application, **Hot Tub Assistant**, that helps you set reminders, store your shopping list, and more! Learn more at [www.hottubassistant.com](http://www.hottubassistant.com).